Structural Engineering Guidance No. 11-01

Date: January 3, 2011

Distribution: All Engineering Resources

SUBJECT: REVISE AND ADD NEW STRENGTHENING EXISTING STRINGERS SPECIAL SHEET

Contact: Gregory Sanders

EPG Status: No Revisions Needed

Special Sheet Status: Add New after Revision Completed

Effective Date: Immediately For All Jobs

Duration: Active for 1 year

Guidance:

An error was discovered on a nonstandardized detail sheet used for showing strengthening plate details for wide flanges used commonly on rehabilitation bridge plans.

Replace “ASTM A706” with “ASTM A709”.

This sheet has been captured and revised for future use. It may be found and used with modifications in T:\br-proj\A\_Development\DS Special Sheets or alternatively on the DS Webpage under Special Sheets.

Suggestions and recommendations concerning this guidance or procedure should be directed to the Development Section for review and updating the Engineering Policy Guide.